Supporting Document for Electrical Hazards in park.

1. Circuit Breaker Panel Boxes Open - Doors open; no door locks allowing public removal of circuit breakers and possible public contact with live electrical wiring (5 locations).

2. Electrical Wiring Junction Boxes Uncovered - Open, no covers allowing possible public contact with live electrical wiring (5 locations)

3. Electrical Wiring Not Enclosed in Conduit - Live, exposed electrical wiring allowing possible public contact (5 locations)

4. Smashed Conduit - Smashed PVC conduit (on the ground) with exposed live electrical wiring allowing possible public contact (1 location)